CTE Frameworks - Auto Collision Equipment List

## Equipment includes:

* Self-piercing rivet gun
* ¼ inch structural rivet gun
* Torque wrench
* Plasma cutter
* Dustless sanding system
* Computer-aided estimating software
* Diagnostic scan tool
* Digital camera
* Factory recommended repair procedures software
* Aluminum dent repair station (including hammers, dollies, stud weld-on tool and pulling equipment, heat gun, non-contact thermometer)
* Steel stud weld-on tool
* Plastic airless welder
* Plastic nitrogen welder (A+)
* Paintless dent repair equipment
* OEM recommended squeeze type resistance spot welder
* Aluminum pulse welder
* Silicon bronze pulse welder
* Welding fume extractor/ventilation system
* Dedicated frame machine
* 3-D Computer aided measuring system
* Wheel alignment equipment
* Tire mount
* Wheel balance machine
* 134A Air condition servicing machine
* Electronic battery charger
* Digital volt ohm meter
* Battery jumper pack
* Hybrid/electric vehicle servicing equipment
* 1234YF Air condition servicing machine
* Headlight aiming equipment
* Advanced driver assistance systems calibration equipment
* OSHA Compliant heated spray booth
* Fresh air respirator system
* Gun washer to clean both solvent and waterborne materials
* Color corrective light
* Spectrophotometer
* Pressure washer
* Carpet extractor/steamer