Carpentry Equipment List

## Examples include and must meet industry standards:

* Computer lab
* Hand tools (hammers, chisels, hand saws, planes, screwdrivers, squares, tape measures, prybars, catspaws, files, pliers, aviation snips)
* Power tools (circular saw, reciprocating saw, Sabre saw, table saw, miter saw, band saw, coping saw, thickness planer, jointer, drill press, portable drill, impact driver, router, orbital sander, belt sander, drywall/decking screw gun, air compressor)
* Pneumatic tools (air hoses, framing nail gun, finish nail gun, siding nail gun, roofing nail gun, flooring staple gun, narrow and wide crown staple guns)
* Extension ladders
* Step ladders
* Copies of a project plan
* Architect scales
* Relevant code books
* Product samples
* Product literature
* Carpentry textbook
* Pipe staging
* Wall brackets with guardrail post
* Roof brackets
* Baker staging, aluminum pole pump staging with safety net and end rails
* Body harness
* Safety rope system
* Retractable lanyard
* OSHA stamped wood planks
* Portable air compressor
* Pneumatic framing nailers
* Extension cords
* 6’ Level
* Rolling baker staging
* Cordless impact driver
* 6” Hand clamps
* Rotary laser level